Infoscreen Instructions

Felix Stoltenberg

[felix.elias.stoltenberg@gmail.com](mailto:felix.elias.stoltenberg@gmail.com)  
<https://github.com/Feriixu/RaspiInfoscreen>

horizontale Linie

# Requirements

* Raspberry Pi with Raspian Full (preferably; not tested with other dists)
* Micro SD Card
* Power supply (or power from the TV / display)
* HDMI Card (if raspi doesn’t have HDMI output)
* Ethernet Card / WiFi dongle (if raspi doesn’t have onboard connectivity)
* Optional: Case

# Installation / Setup

1. Enable SSH (for later enabling and disabling of the kiosk script)
2. Setup network connection
3. Copy all files to /home/pi
4. Run kiosk\_setup.sh
5. Edit kiosk.sh and enter the URL’s for Presentation and Personio
6. Reboot
7. Done!

Log in via SSH and run enable\_kiosk.sh / disable\_kiosk.sh for enabling and disabling. (Kiosk is enabled by default after setup)